**Adjustable mirror with handle**

Metallised anthracite handle

Reference: **510202C**

Specification description

Wall-mounted, rectangular, tilting mirror with handle for easy adjustment those in a seated position or in a wheelchair.

For disabled washrooms and combined installation: can be used from a sitting position, for people with reduced mobility, or standing position.

NylonClean lever with anti-bacterial treatment: optimal protection against bacterial development.

Quick and easy to install: simply clip into place.

Anti-theft lock.

Tilting mirror with metallised anthracite tab handle.

Mirror made from 6mm safety glass.

Mirror dimensions: 500 x 600mm.

Can be tilted up to 20°.

Tilting mirror with 30-year warranty.