**LP trough urinal**

Polished satin 304 stainless steel - L. 1800mm - Floor-standing

Reference: **130320**

Specification description

Floor-standing trough urinal, 1800 x 1020 x 300mm.

Bacteriostatic 304 stainless steel.

Polished satin finish.

Stainless steel thickness: 1.2mm.

Rear water inlet.

Supplied with 3 stainless steel rinsers and 3 flexible hoses.

Water saving: optimal rinsing with 0.1 L/sec. per service i.e. 0.3L per use.

Central drainage.

Waste outlet 1½". Supplied with waste and integrated trap (ref. 785000).

Easy to install and maintain thanks to access panels with theft prevention TORX security screws.

Weight: 33.5kg.

Possible to add one or more bacteriostatic 304 stainless steel dividers. Fix directly onto the urinal in the desired location.