**Towel rail**

Ø 20mm, 2 rails

304 white powder-coated stainless steel

Reference: **510790W**

Specification description

Towel rail for bathrooms.

Twin rail designer towel rail.

Robust model.

Tube Ø 20mm and Ø 16mm, length 600mm.

White powder-coated bacteriostatic 304 stainless steel.

Wall-mounted towel rail with concealed fixings.

30-year warranty.