**Shock-resistant trigger-operated hand spray**

With adjustable jet

Reference: **433011**

Specification description

Trigger-operated hand spray with adjustable jet and shock-resistant protection.

Ergonomic grip with protection is easy to grip.

Internal mechanism will withstand chemical products.

Maximum temperature: 50°C.

Maximum pressure: 12 bar.

Possible to lock the trigger in the open position using a collar.

Connection to the flexible via removable rapid push-fit connector.

30-year warranty.