**Mechanical basin mixer**

Wall-mounted mixer with swivel spout L .200mm, sculptured lever

With offset STOP/CHECK connectors

Reference: **2445**

Specification description

Wall-mounted mechanical basin mixer.

Mechanical mixer with flat, swivelling under spout L. 200mm with hygienic flow straightener.

Spout suitable for fitting a BIOFIL point-of-use filter.

Securitouch thermal insulation prevents burns.

Ø 40mm standard ceramic cartridge with pre-set maximum temperature limiter.

Body and spout with smooth interiors and low water volume.

Flow rate 5 lpm 3 bar.

Chrome-plated brass body.

Sculptured control lever.

Mixer with 150mm centres, supplied with offset STOP/CHECK wall connectors M1/2" M3/4" ideal for hospitals.

Recommended installation height: 110 - 200mm above the basin surface.

Mechanical mixer ideal for healthcare facilities, retirement and care homes. hospitals and clinics.

Mixer suitable for people with reduced mobility.

Wall-mounted mixer with 30-year warranty.