**HIGHFLOW high-speed hand dryer**

Air pulse

White powder-coated 304 stainless steel

Reference: **510622W**

Specification description

HIGHFLOW air pulse hand dryer.

Robust model.

Lit central nozzle concentrates pulsed air onto hands at 230km/h.

High speed electrical hand dryer: dries in 10 to 12 seconds.

Choice of warm or cold air via concealed switch.

Automatic hand dryer, infrared detection.

Intelligent technology: stops automatically when hands are removed.

Anti-blocking: stops automatically if used continuously for more than 60 seconds.

Bacteriostatic powder-coated 304 stainless steel.

Easy to clean: one-piece cover.

Stainless steel thickness: 1mm.

Airflow: 39 l/second.

Air speed: 230km/h.

Low energy consumption: 1,350W.

220-240V~ / 50 Hz.

Noise level: 82 dBA.

Dimensions: 175 x 238 x 267mm.

Weight: 4kg.

Class I, IP23.

CE marked.

3-year warranty.