**TEMPOFLUX urinal valve**

Time flow 3 seconds. For DELABIE FINO urinal

Angled. Soft-touch operation

Reference: **778759**

Specification description

Exposed time flow urinal valve:

For DELABIE FINO urinals.

Soft-touch operation.

Time flow pre-set at ~3 seconds.

Flow rate pre-set at 0.15 L/sec at 3 bar, can be adjusted up to 0.3 L/sec.

Innovative stopcock and flow rate adjustment system integrated in the wall plate (patented).

Compatible with rain water.

Complies with European standard EN 12541 (class II acoustic level).

Chrome-plated solid brass body M½".

With chrome-plated neck tube.

Angled for recessed inlet.

Suitable for people with reduced mobility.

30-year warranty.