**Be-Line® wall-mounted toilet brush set**

Model with anti-theft lock for fixing

304 stainless steel metallised anthracite

Reference: **4048C**

Specification description

Wall-mounted Be-Line® toilet brush set.

Wall-mounted robust toilet brush set with anti-theft lock for fixing.

Bacteriostatic metallised anthracite powder-coated 304 stainless steel.

Easy to clean: plastic bowl can be removed from above.

Plastic bowl with reservoir: prevents the brush from sitting in stagnant water and splashing when next used.

Stainless steel thickness: 1mm body.

Dimensions: Ø 90 x 330mm.

30-year warranty.