**Twin hole pre-rinse set with mixer**

With bib tap

Black flexible hose L. 95cm and ergonomic controls

Reference: **5633UK**

Specification description

Complete pre-rinse set with bib tap.

Deck-mounted twin hole mixer with 180mm centres with:

- Valve heads with reinforced mechanisms with ergonomic control levers.

- Offset inlet connections with M1/2" tails.

Bib tap with:

- Swivelling, tubular spout L. 200mm.

- 25 lpm full flow rate achieved within the first 90°.

- Valve head with reinforced mechanism with ergonomic control lever.

Black, scale-resistant M1/2" hand spray with adjustable jet and 9 lpm flow rate at the outlet.

Black, reinforced, food-grade flexible hose L. 0.95m.

3/4" brass column.

Adjustable wall bracket.

Stainless steel spring guide.

30-year warranty.

These pre-rinse models can be installed close to the splashback.