**Hygienic BIOSAFE outlet M24/100**

50 units

Reference: **923024.50P**

Specification description

BIOSAFE free flow hygienic outlet M24/100 for basin taps/mixers.

No grid or partitions in contact with water.

Flow rate 5 lpm.

No water stagnation is possible in internal parts reducing bacterial development.

Made of Hostaform® reducing scale build-up.

Chrome-plated brass ring.

Supplied in packs of 50.

Can only be installed on a tap or mixer with an already limited flow rate in order to maintain a good flow without splashing.