**SECURITHERM EP pressure-balancing basin mixer**

High single hole, single control mixer with EP cartridge

Mixer with removable, disposable swivelling spout

Reference: **2871T1EP**

Specification description

Deck-mounted, tall basin mixer with SECURITHERM pressure-balancing.

Single hole, single control mixer with high, swivelling spout H. 180mm L. 180mm.

Mechanical mixer supplied with 1 removable disposable spout.

Anti-scalding safety: reduced HW flow rate if CW supply fails (and vice versa).

Ø 35mm ceramic cartridge with pressure-balancing and pre-set maximum temperature limiter.

Body and spout with smooth interiors (limits bacterial development).

Thermal shocks are easy to undertake without removing the control lever or shutting off the cold water supply.

Flow rate regulated at 5 lpm.

Hygiene lever L. 185mm for touch-free control.

Chrome-plated brass body and base.

PEX flexibles F3/8" with filters and non-return valves.

Fixing reinforced via 2 stainless steel rods.

Mechanical mixer ideal for healthcare facilities, retirement and care homes, hospitals and clinics.

Single control mixer suitable for people with reduced mobility.

Mixer with 30-year warranty.