**SECURITHERM EP pressure-balancing basin mixer**

Tall single hole single control mixer with EP pressure-balancing

Mechanical mixer with swivelling spout H.165 L.220

Reference: **2564T2EP**

Specification description

Deck-mounted basin mixer with SECURITHERM pressure-balancing.

Single hole, single control mixer with swivelling spout H. 165mm L. 220mm.

Tall mixer with BIOSAFE hygienic outlet suitable for fitting a BIOFIL point-of-use filter.

Anti-scalding safety: HW flow reduces if CW supply fails (and vice versa).

Ø 35mm ceramic cartridge with pressure balancing and pre-set maximum temperature limiter.

Body and spout with smooth interiors (reduces bacterial development).

Thermal shocks are possible without removing the control lever or shutting off the cold water.

Flow rate regulated at 5 lpm.

Chrome-plated brass body and base.

Hygiene control lever L. 185mm requires no manual contact.

PEX flexibles F3/8" with filters and non-return valves.

Fixing reinforced via by 2 stainless steel rods.

Pressure-balancing mixer ideal for use in healthcare facilities, retirement and care homes, hospitals and clinics.

Single hole mixer suitable for people with reduced mobility.

Mixer with 30-year warranty.