**SPORTING 2 shower panel**

Electronic mains supply, rain-effect spray

Top or concealed inlet, anodised aluminium

Reference: **714800**

Specification description

Electronic shower panel:

Anodised aluminium and chrome-plated satin finish panel.

Adjustable connector for top or back inlets.

Slimline structure with concealed fixings.

Mains supply 230/6V.

Infrared presence detection. Shower starts when hand is moved towards the sensor (detection distance ~4cm).

Shuts off voluntarily or automatically after ~60 seconds.

Duty flush (~60 seconds every 24 hours after the last use).

Flow rate 6 lpm at 3 bar, comfortable rain-effect spray.

Tamperproof, scale-resistant fixed shower head with automatic flow rate regulation.

Adjustable spray.

Accessible filter.

Integrated stopcock.

M½" connection for mixed water supply.

Suitable for people with reduced mobility.

30-year warranty.