**TEMPOSOFT 2 time flow tap**

Soft-touch operation

Wall-mounted L.110mm

Reference: **741500**

Specification description

Wall-mounted time flow basin tap:

Soft-touch operation.

Time flow ~7 seconds.

Flow rate pre-set at 3 lpm at 3 bar, can be adjusted from 1.4 to 6 lpm.

Tamperproof scale-resistant flow straightener.

Solid chrome-plated brass body M½". L. 110mm.

Supplied with red and blue markers.

Suitable for people with reduced mobility.

30-year warranty.