**BIOSAFE mechanical basin mixer**

Single hole mechanical mixer with no spout, H. 95mm L. 110mm

Without pop-up waste

Reference: **2621**

Specification description

Deck-mounted mechanical basin mixer.

Single hole mechanical mixer H. 95mm L. 110mm.

No spout: hygienic flow straightener integrated into the body.

Securitouch thermal insulation prevents burns.

Ø 35mm ceramic cartridge with pre-set maximum temperature limiter.

Thermal shocks are possible without removing the control lever or shutting off the cold water supply.

Mixer body with smooth interior and very low water volume (limits bacterial development).

Flow rate regulated at 4 lpm.

Solid control lever.

No pop-up waste.

PEX flexibles F3/8", rotating unions.

Fixing reinforced by two stainless steel rods.

Mechanical mixer ideal for healthcare facilities, retirement and care homes, hospitals and clinics.

Single hole mixer suitable for people with reduced mobility.

Mixer with 30-year warranty.

Also available with copper tails.