**Deck-mounted single hole mixer - 60 lpm**

Swivelling spout H. 255mm L. 200mm

For plunge sinks

Reference: **5650T2**

Specification description

Deck-mounted single hole catering mixer.

Swivelling tubular spout H. 255mm L. 200mm with hygienic flow straightener.

Ceramic cartridge Ø 45mm.

Flow rate 60 lpm at 3 bar.

Spout with smooth interior.

Slimline control lever.

Chrome-plated brass body and spout.

Soldered copper pipe water inlets.

Reinforced fixing.

30-year warranty.