**Wall-mounted SD drinking fountain**

With bubbler tap and swan neck tap

Reference: **180820**

Specification description

Wall-mounted drinking fountain.

Bacteriostatic 304 stainless steel.

Polished satin finish.

Stainless steel thickness: 1.2mm.

Rounded edges prevent injury.

Supplied with a bubbler tap: chrome-plated, instant shut-off with flow rate adjustment, inlet M⅜".

Supplied with a swan neck tap for filling bottles and flasks: chrome-plated body and stainless steel spout, instant shut-off with adjustable flow rate, connector M⅜".

Flat perforated waste, without screws: easy to clean and vandal-resistant.

Waste outlet 1¼".

Supplied with fixing elements.

Weight: 3kg.

30-year warranty.