**UNITO countertop washbasin**

Polished satin 304 stainless steel - Countertop installation

With Ø 35mm central tap hole

Reference: **121810**

Specification description

Countertop washbasin, 395 x 405mm.

Suitable for use with wall-mounted or extended mixer/tap.

Bacteriostatic 304 stainless steel. Polished satin finish.

Stainless steel: 1.2mm.

Rounded edges prevent injury.

With Ø 35mm central tap hole.

Supplied with 1¼" waste.

Without overflow.

CE marked. Complies with European standard EN 14688.

Weight: 3.6kg.

30-year warranty.