**TEMPOMATIC 4 urinal valve**

Electronic with integrated batteries

Reference: **430P006**

Specification description

Recessed electronic urinal valve:

123 6V Lithium battery-operated.

Satin finish stainless steel wall plate 145 x 145mm with integrated electronics.

Recessing housing:

- Hydraulic connection to the outside.

- Adjusts to all types of installation (rails, solid walls, panels).

- Compatible with wall finishes 10 - 120mm (while maintaining the minimum recessing depth of 105mm).

- Integrated solenoid valve is accessible from the front.

- TEMPOMATIC 4 urinal valve F½" is compatible with sea water and grey water.

Detection delay is 10 seconds.

3 programmes (rinsing volume can be set according to urinal type).

High-frequency mode (exclusive to DELABIE):

- Short rinse after each user.

- Additional rinse at the end of the busy period.

Hygienic duty flush every 24 hours (can be adjusted to 12 hours or OFF) after the last use: prevents vacuums.

Flow rate pre-set at 0.3 L/sec. at 3 bar.

Suitable for people with reduced mobility.

30-year warranty.