**HIGHFLOW automatic air pulse hand dryer in matte black**

Air pulse

Matte black 304 stainless steel

Reference: **510622BK**

Specification description

HIGHFLOW air pulse hand dryer.

Robust model.

Lit central nozzle focuses the pulsed air onto hands at over 230km/h.

High speed: dries in 10 - 12 seconds.

Choice of warm or cold air via a concealed switch.

Infrared automatic activation.

Intelligent technology: stops automatically when hands are removed.

Anti-blocking: stops automatically if used continuously for more than 60 seconds.

Electrical hand dryer made from matte black bacteriostatic 304 stainless steel.

Easy to clean: one-piece cover.

Stainless steel thickness: 1mm.

Dimensions: 175 x 238 x 267mm.

Weight: 4kg.

Airflow: 39 l/second.

Air speed: 230 km/h.

Low energy consumption: 1,350W.

220-240 V~ / 50 Hz.

Noise level: 82 dBA.

Class I, IP23.

CE marked.

Automatic hand dryer with a 3-year warranty.