**BIOSAFE hygienic outlet M24/100**

1 per pack

For 2620 range

Reference: **926024**

Specification description

BIOSAFE free flow hygienic outlet M24/100 for basin taps/mixers in the 2620 range.

No grid or partitions in contact with water.

Flow rate 5 lpm.

No water stagnation is possible in internal parts reducing bacterial development.

Made of Hostaform® reducing scale build-up.

Chrome-plated brass ring.

Supplied individually.

Can only be installed on a tap or mixer with an already limited flow rate in order to maintain a good flow without splashing.