**Single hole pre-rinse set with mixer**

With bib tap and swivelling telescopic spout

Black flexible with scale-resistant hand spray

Reference: **5832**

Specification description

Complete pre-rinse set with bib tap.

Suitable for intensive use in professional kitchens.

Single hole deck-mounted mixer with:

- valve heads with reinforced mechanism and ergonomic controls.

- F3/8" flexible hoses and non-return valves.

- fixing reinforced by 2 threaded rods and back nuts.

Bib tap with swivelling, tubular spout L. 200mm.

- 20 lpm full flow rate achieved within 90° turn.

- valve head with reinforced mechanism and ergonomic control.

Black hand spray with adjustable jet and 10 lpm flow rate at the outlet (ref. 433009).

Scale-resistant hand spray with shock-resistant tip.

Reinforced, food-grade black flexible hose L. 0.95m.

3/4" brass column.

Adjustable wall bracket.

Stainless steel spring guide.

30-year warranty.