**Recessed waterproof housing for TEMPOMIX 3 basin controls**

Waterproof, kit 1/2

Recessed

Reference: **794BOX3**

Specification description

Waterproof recessed housing for TEMPOMIX 3 basin water controls, kit 1/2:

- Collar with waterproof seal.

- Hydraulic connection from the outside and maintenance from the front.

- Adjusts to all types of installations (rails, solid walls, panels).

- Compatible with wall finishes 10 - 120mm (while maintaining the minimum recessing depth of 93mm).

- Suitable for standard or "pipe in pipe" supply.

- Stopcocks and flow rate adjustment, filters, non-return valves and cartridge are all integrated and accessible from the front.

- TEMPOMIX 3 single control mixer F½".

- Supplied in 2 kits: secure system flush without sensitive elements.

30-year warranty.

Order with control plates references 794200 or 794250.