**TEMPOMIX 3 shower kit**

Single control time flow, kit 2/2

Recessed waterproof, chrome-plated metal control

Reference: **794219**

Specification description

Recessed time flow shower kit with soft-touch operation, kit 2/2:

Tamperproof chrome-plated metal control plate 160 x 160mm.

Operation and temperature selection on the control button.

Maximum temperature limiter (can be adjusted by installer).

Time flow ~30 seconds, can be adjusted.

Soft-touch operation.

Flow rate 6 lpm at 3 bar.

Chrome-plated, tamperproof, scale-resistant ROUND shower head with automatic flow rate regulation.

Suitable for people with reduced mobility.

30-year warranty.

Order with recessed waterproof housing ref. 794BOX1.