**SECURITHERM time flow shower mixer**

Thermostatic time flow, kit 2/2

Recessed

Reference: **792218**

Specification description

Recessed thermostatic time flow shower mixer:

Tamperproof satin finish stainless steel control plate 195 x 220mm.

Anti-scalding failsafe: automatic shut-off if cold water fails.

Anti-cold showers function: automatic shut-off if hot water fails.

Temperature can be adjusted from 32 to 40°C, pre-set at 38°C.

Soft-touch operation.

Time flow ~30 seconds.

Flow rate set at 9 lpm at 3 bar.

Concealed fixings, stopcocks M½".

Integrated non-return valves and filters.

Chrome-plated Bayblend® control knob.

Suitable for people with reduced mobility.

30-year warranty.

Order with recessed housing ref. 792BOX.