**RAINY shower head**

Rain-effect shower head, cross wall

Scale-resistant

Reference: **708200**

Specification description

Fixed shower head.

Flow rate 6 lpm at 3 bar.

A higher flow rate can be achieved: remove flow rate regulator.

Scale-resistant head with nozzles, ligature-resistant.

Soft rain-effect flow engulfs user.

Chrome-plated metal.

Easy installation system: install the connection in the wall and then clip the shower head to it.

Inlet F½".

Shower head for cross wall installation (maximum partition thickness: 230mm).

30-year warranty.