**TEMPOMIX time flow shower mixer**

Single control time flow, kit 2/2

Recessed waterproof, ROUND shower head

Reference: **790219**

Specification description

Recessed time flow shower mixer kit, kit 2/2 :

Tamperproof bright polished stainless steel wall plate 160 x 220mm.

TEMPOMIX ¾" single control mixer.

Ligature-resistant collar.

Temperature control and operation on the push-button.

Maximum temperature limiter (can be adjusted by the installer).

Time flow ~30 seconds, soft-touch operation.

Flow rate 6 lpm at 3 bar.

Chrome-plated, tamperproof ROUND shower head with scale-resistant nozzle and automatic flow rate regulation.

Concealed fixings, stopcocks M½".

Chrome-plated metal control.

Integrated non-return valves and filters.

30-year warranty.

Order with waterproof housing ref. 790BOX