**TEMPOFIX 3 wall-mounted frame system for WCs**

For time flow or battery-operated electronic valve - Ø 110mm outlet

Wall-mounted, for walls from 10 to 120mm

Reference: **564060DE**

Specification description

Wall-mounted frame system for wall-hung WCs, kit 1/2:

Black powder-coated steel frame:

- For fixing to load-bearing walls.

- Frame height can be adjusted from 0 - 200mm (with 1m mark).

- Compatible with solid walls from 10 - 120mm.

- Ø 32mm flush tube with Ø 55mm connection washer.

- ABS soil pipe, Ø 110mm HDPE outlet with waterproof seal, with 2 setting positions.

Recessed waterproof housing: flush system without cistern, directly connected to pipework.

- Compatible with electronic or time flow valves for WCs.

- Compatible with CR123 Lithium 6V battery.

- Backflow prevention device inside the housing.

- Integrated stopcock and flow rate regulation.

Supplied pre-mounted.

30-year warranty.

Order with control plate references 464006, 465006, 763000, 763030, 763040 or 763041.