**Self-supporting TEMPOFIX 3 frame system for WCs**

For TEMPOFLUX 2 time flow valve - Outlet Ø 100mm

Self-supporting, for walls from 30 to 60mm

Reference: **578405**

Specification description

Self-supporting frame system for wall-hung WCs, kit 1/2:

Black powder-coated steel frame:

- With large feet for fixing to load-bearing floors.

- Frame height can be adjusted from 0 - 200mm (with 1m mark).

- For semi-thick wall finishes from 30 to 60mm.

- Ø 32mm flush tube with Ø 55mm connection washer.

- Ø 100mm soil pipe and ABS collar with waterproof seal, with 2 settings positions.

Fitted with a TEMPOFLUX 2 time flow direct flush:

- Flush system without cistern: directly connected to pipework.

- Vacuum breaker.

- Integrated stopcock and flow rate/volume adjuster.

- Solid brass body and shock-resistant, scale-resistant mechanism.

- In-line inlet M¾".

- Upstream supply pipes: minimum Ø 20mm required at all points (including connectors).

- Base flow rate: 1L/sec at 1 bar dynamic pressure.

- Compatible with rain water.

Delivered pre-mounted.

30-year warranty.

Order with control plate references 578222 or 578212.