**Electrovanne**

For TEMPOMATIC multi-urinals

M3/4" - 12V - With filter

Reference: **429101**

Specification description

Solenoid valve with filter.

For TEMPOMATIC urinals.

Unions M3/4".

Works with a 12V power supply.

Dimensions: 62 x 49,3mm.