**Solenoid valve**

For TEMPOMATIC 3 and TEMPOMATIC 4 basin controls

With flow rate adjustor - M28 - 6V

Reference: **479650**

Specification description

Piston operated solenoid valve with flow rate adjustor.

For TEMPOMATIC 3 basin controls (from May 2023).

For TEMPOMATIC 4 basin controls (with flow rate regulator).

Works with a 6V power supply.

Dimensions: 36 x 38mm, M28 x 1.5.