**Wall-hung S21 S WC pan**

Matte black 304 stainless steel

Reference: **110310BK**

Specification description

Wall-hung WC pan.

Compatible with all standard frame systems available on the market.

Elegant and simple design.

Bacteriostatic 304 stainless steel. Stainless steel thickness: 1.5mm.

Matte black Teflon® finish.

One-piece pressed WC bowl, seam-free for easy maintenance and better hygiene.

Concealed perimetral flushing rim.

Horizontal water inlet: Ø 55mm.

Horizontal waste outlet: Ø 100mm.

Water saving: works with 4L or more of water.

Shrouded pan.

Pre-drilled holes for fixing the toilet seat. Supplied with stainless steel blanking caps when installed without toilet seat lid.

Quick and easy to install from the front thanks to a stainless steel mounting frame.

Supplied with fixing plate and 6 theft prevention TORX security screws.

CE marked. Complies with European standard EN 997 for 4L flush.

Weight: 11kg.

30-year warranty