**Ø40mm ceramic pressure balancing EP cartridge with base**

Cartridge with base

No flow rate limiter

Reference: **N252**

Specification description

Ø40mm ceramic pressure balancing EP cartridge with base.

For deck-mounted basin mixer ranges:

- 2211EP, 2211LEP

- 2520EP, 2520LEP, 2520TEP / 2521EP, 2521TEP, 2521LEP

- 2720LEP, 2720TEP / 2721TEP, 2721LEP (for models sold before 12/2022)

- 2820LEP, 2820TEP (for models sold before 05/2023)

-2821TEP, 2821LEP

- 2565TxEP (for models sold before 03/2020)

For wall-mounted basin mixer ranges:

- 2445EP, 2446EP, 2455EP, 2456EP

For shower mixer ranges:

- 2239EP, 2239EPS

- 2539EP, 2539EPS

- 2739EP, 2739EPS, 2739TEP, 2739TEPS