**Electronic control unit**

For TEMPOMATIC basins

Battery-operated

Reference: **495446BC**

Specification description

Electronic control unit.

Electronic unit for TEMPOMATIC basin mixers and taps.

With duty flush feature.

Works with a 6V battery supply.

Dimensions: 110 x 75 x 41mm.