**TEMPOFLUX 3 AB side control flush system**

Time flow valve AB, soft-touch side control, recessed

3L/6L dual flush side plate -satin stainless steel

Reference: **763300**

Specification description

Flush system without cistern: directly connected to pipework.

Satin stainless steel access plate to mechanism 186 x 186mm.

Satin stainless steel time flow control plate and chrome-plated buttons 90 x 90mm.

Control plate is installed manually via hidden screws.

Recessed waterproof housing:

- Collar with waterproof seal.

- Hydraulic connection to the outside and maintenance from the front.

- Compatible with wall finishes from 10 - 120mm (while maintaining the minimum recessing depth of 93mm).

- Suitable for standard or "pipe-in-pipe" supply.

- Stopcock and flow rate adjustment are integrated and accessible from the front.

- Cartridge and filter are accessible from the front.

- TEMPOFLUX 3 F¾" valve compatible with sea water, rain water and grey water.

- Backflow prevention device inside the housing.

Soft-touch operation.

AB anti-blocking system: water will flow only when the push-button is released.

3L/6L dual flush can be adjusted to 2L/4L.

Outlet connection for PVC tube Ø26/32mm.

Acoustic level complies with European standard EN 12541 class II.

Upstream supply pipes: minimum Ø 20mm required at all points (including connectors).

Base flow rate: 1 L/sec at 1 bar dynamic pressure.

Suitable for rimless WC pans without flow rate regulation.

Suitable for people with reduced mobility

30-year warranty.