**Time flow cartridge**

For TEMPOGENOU

Time flow ~7 seconds

Reference: **743305**

Specification description

Knee-operated time flow cartridge for non-manual controls.

For TEMPOGENOU time flow mixers and taps.

Cartridge for cross wall TEMPOSTOP mixers and taps with lever.

Time flow ~7 seconds.

Adjustable flow rate from 1.4 to 6 lpm.