**Mirror cabinet with 4 functions**

Mirror, hand dryer, soap dispenser and electronic tap

Matte black and st. steel finish, 304 - 800mm

Reference: **510204**

Specification description

Mirror cabinet with 4 functions: mirror, electronic tap, soap dispenser and electrical hand dryer.

304 stainless steel designer cabinet with a matte black melamine finish.

Touch-free for improved hygiene: soap dispenser, tap and hand dryer are activated automatically when hands are detected by infrared sensor.

Quick and easy to install:

- A single electrical connection for all the elements: mains supply with 230V / 50-60Hz.

- Connects to the water supply from the top or from inside the cabinet.

- Water connection in M3/8".

- Concealed fixings. Mirror cabinet supplied with stainless steel screws for concrete or reinforced wood.

- Adjustable hinges.

Unit with 4 functions:

4mm thick glass mirror and black glass strip with illuminated pictograms.

Automatic soap dispenser:

- No-waste pump dispenser

- Large capacity tank: 5 litres.

- Suitable for vegetable-based liquid soap with a maximum viscosity of 3,000 mPa.s or specific foam soap.

Electronic basin tap\*:

- Reduced stagnation solenoid valve.

- Flow rate pre-set at 3 lpm at 3 bar, can be adjusted from 1.4 to 6 lpm.

- Scale-resistant flow straightener.

- Duty flush (~60 seconds every 24 hours after the last use).

- Stopcock.

Air-pulse hand dryer:

- High-speed.

- Pulsed air at 360km/h. Airflow: 36 l/second.

- Low energy consumption: 704W.

- Noise level: 74 dBA.

- Class I, IP23.

- 3-year warranty.

Basin lit by the LED strip.

Vandal-resistant model with standard DELABIE key.

Anti-blocking: stops automatically if used continuously.

Internal storage shelf.

Several cabinets can be installed side-by-side to create a mirror wall: linking screws are provided.

Dimensions: 800 x 223 x 1,000mm.

Weight: 39kg.

Mirror cabinet with 30-year warranty.

CE marked.

\* We recommend a PREMIX mixer.