**Time flow cartridge**

Mechanism for TEMPOSTOP urinal

Time flow ~7 seconds

Reference: **743645**

Specification description

Time flow cartridge for TEMPOSTOP urinal valves.

For 3/4" urinal valves.

Time flow ~7 seconds.

Flow rate can be adjusted.