**Time flow cartridge**

Mechanism for TEMPOFLUX urinal

Time flow ~7 seconds

Reference: **743777**

Specification description

Time flow cartridge for TEMPOFLUX urinal valves.

For urinal valves with soft-touch operation.

For 1/2" urinal valves.

Time flow ~7 seconds.

Flow rate can be adjusted.