**Thermostatic mixing valve repair kit**

For PREMIX COMPACT thermostatic mixing valve

For mixed water distribution from 30 - 60°C.

Reference: **753733**

Specification description

Repair kit for PREMIX COMPACT thermostatic mixing valve.

Original design.

Cartridge with thermostatic cell.

Anti-scalding safety: shuts off automatically if the cold or hot water supply fails.