**Time flow cartridge**

For TEMPOMIX 3 basin mixers

Time flow ~7 seconds

Reference: **743794**

Specification description

Time flow cartridge for TEMPOMIX 3 basin mixers.

For TEMPOMIX 3 basin mixers type 794XXX.

Time flow ~7 seconds.

Flow rate can be adjusted from 1.4 - 6 lpm.