**BINOPTIC 2 electronic tap**

Batteries, deck-mounted, H. 100mm

Smooth interior spout, chrome-plated

Reference: **373116**

Specification description

Deck-mounted chrome-plated electronic basin tap:

Operated by CR123 Lithium 6V batteries.

Reduced stagnation solenoid valve and electronic unit integrated into the body of the tap.

Flow rate pre-set at 3 lpm at 3 bar, can be adjusted from 1.4 to 6 lpm.

Scale-resistant aerator.

Adjustable duty flush (~60 seconds every 24 hours after the last use).

Stainless steel tap, 100mm high for inset basins.

Presence detection sensor at the end of the spout optimises detection.

PEX flexible with filter.

Fixing reinforced by 2 stainless steel rods.

Anti-blocking security.

Smooth interior spout with low water volume (limits bacterial niches).

Set detection range, duty flush and launch thermal shocks manually.

Suitable for people with reduced mobility.

30-year warranty.