**BINOPTIC MIX 2 electronic basin mixer**

Mains supply, deck-mounted, H. 100mm, Bluetooth®

Smooth interior spout, chrome-plated, std lever

Reference: **473110E**

Specification description

Deck-mounted chrome-plated electronic basin mixer:

230/6V mains supply.

Reduced stagnation solenoid valve and electronic unit integrated into the body of the mixer.

Flow rate pre-set at 3 lpm at 3 bar, can be adjusted from 1.4 to 6 lpm.

Scale-resistant aerator.

Adjustable duty flush (~60 seconds every 24 hours after the last use).

Stainless steel mixer, 100mm high for inset basins.

Presence detection, sensor at the end of the spout optimises detection.

PEX flexibles F3/8" with filters and non-return valves

Fixing reinforced by 2 stainless steel rods.

Anti-blocking security.

Smooth interior spout with low water volume (limits bacterial niches).

Side temperature control with adjustable maximum temperature limiter.

Set detectiion distance, duty flush and launch thermal shocks manually.

Bluetooth® version: advanced settings and operating data download via DELABIE Connect app.

Suitable for people with reduced mobility.

30-year warranty.