**BINOPTIC MIX 2 electronic basin mixer**

Mains supply, deck-mounted, stopcocks, H. 100mm

Smooth interior spout, satin, standard lever

Reference: **47300015**

Specification description

Deck-mounted satin finish electronic basin mixer:

230/6V mains supply.

Reduced stagnation solenoid valve and electronic unit integrated into the body of the mixer.

Flow rate pre-set at 3 lpm at 3 bar, can be adjusted from 1.4 to 6 lpm.

Scale-resistant aerator.

Adjustable duty flush (~60 seconds every 24 hours after the last use).

Stainless steel mixer, 100mm high for inset basins.

Sensor at the end of the spout optimises presence detection.

PEX flexibles Ø 15mm for compression fittings with stopcocks, filters and non-return valves.

Fixing reinforced by 2 stainless steel rods.

Anti-blocking security.

Smooth spout interior with low water volume (reduces bacterial development).

Side temperature control with adjustable maximum temperature limiter.

Set presence detection range, duty flush and launch thermal shocks manually.

Suitable for people with reduced mobility.

30-year warranty.