**TEMPOMATIC 5 electronic basin tap**

Batteries, wall-mounted

Spout, L. 150mm

Reference: **449406**

Specification description

Wall mounted electronic basin tap:

Operated by CR123 6V Lithium batteries.

Reduced stagnation solenoid valve and electronics integrated into the body of tap.

Flow rate pre-set at 3 lpm, can be adjusted from 1.4 to 6 lpm.

Scale-resistant flow straightener.

Duty flush (~60 seconds every 24 hours after last use).

Active infrared presence detection sensor at the end of the spout optimises detection.

Chrome-plated metal body.

Wall mounted.

Anti-blocking security.

Suitable for people with reduced mobility.

30-year warranty.