**TEMPOMATIC 5 electronic basin tap**

Batteries, cross wall

For panels, W.230mm

Reference: **449416**

Specification description

Wall mounted electronic basin tap:

Operated by CR123 6V Lithium batteries.

Reduced stagnation solenoid valve and electronics integrated into the body of tap.

Flow rate pre-set at 3 lpm, can be adjusted from 1.4 to 6 lpm.

Scale-resistant flow straightener.

Duty flush (~60 seconds every 24 hours after last use).

Presence detection sensor at the end of the spout optimises detection.

Chrome-plated stainless steel body, L. 150mm.

Cross wall installation for wall mounting.

Anti-blocking security.

Side temperature control with standard lever and adjustable maximum temperature limiter.

Suitable for people with reduced mobility.

30-year warranty.