**TEMPOMATIC 4 electronic shower valve**

Battery 6V - kit 2/2

Recessed

Reference: **443218**

Specification description

Recessed electronic shower valve, kit 2/2:

Tamperproof chrome-plated metal control plate Ø 149mm.

TEMPOMATIC 4 electronic valve M1/2" for mixed water supply.

Battery-operated with CR123 6V Lithium batteries.

Infrared presence detection sensor. Shower starts when hand is moved towards the sensor (detection distance ~4cm).

Shuts off voluntarily or automatically after ~60 seconds.

Duty flush (~60 seconds every 24 hours after the last use).

Flow rate 16 lpm at 3 bar.

Install in waterproof housing with waterproof collar, filter and stopcock.

Suitable for people with reduced mobility.

30-year warranty.

Order with recessed waterproof housing ref. 443PBOX.