**TEMPOSOFT 2 time flow shower valve**

Kit 2/2

Recessed

Reference: **748218**

Specification description

Recessed time flow shower valve, kit 2/2 :

Tamperproof chrome-plated metal control plate Ø149mm.

For installation in a waterproof housing with: collar with a waterproof seal, filter and stopcock.

TEMPOSOFT 2 M1/2" shower valve; supply with mixed water.

Soft-touch operation.

Time flow ~30 seconds.

Flow rate 16 lpm at 3 bar for the valve only.

Suitable for people with reduced mobility.

30 year warranty.

Order with recessing housing ref. 748BOX.