**Electronic soap dispenser unit for installation behind the mirror**

Liquid soap, foam soap or hydroalcoholic gel dispenser

For installation behind the mirror, mains, 5L tank

Reference: **510203SD**

Specification description

Electronic soap dispenser unit for installation behind a mirror or cabinet.

Touch-free for improved hygiene: soap dispenser is activated automatically when hands are detected by infrared sensor.

- Easy to install: fitted into a cabinet. Fixings on the sides and the back.

- 304 stainless steel support, 1.2 mm thick.

- Mains supply with 100-240V / 6V 50-60 Hz. transformer.

- No-waste pump dispenser.

- Large capacity tank: 5 litres.

- Suitable for vegetable-based liquid soap with a maximum viscosity of 3,000 mPa.s or specific foam soap.

Supplied with self-adhesive pictogram to indicate the location of the soap dispenser on the mirror/cabinet.

Anti-blocking: stops automatically if used continuously.

Dimensions: 230 x 177 x 376mm.

Weight: 1.6 kg.

30-year warranty.

CE.