**TEMPOSTOP time flow shower kit with 2 controls**

Time flow, AB anti-blocking model

Cross wall 200mm, AB, 2 controls

Reference: **747210**

Specification description

Cross wall time flow shower kit:

TEMPOSTOP time flow valve M½".

For wall depths ≤ 200mm.

Time flow ~15 seconds.

Flow rate 6 lpm at 3 bar.

2 controls: 1 mixed water push-button and 1 cold water push-button.

Chrome-plated, tamperproof, ROUND shower head with automatic flow rate regulation.

Chrome-plated metal push-buttons.

Concealed fixing and anti-rotating pin

Threaded rods can be cut-to-size.

AB anti-blocking system: water only flows when push-button is released.

30-year warranty.